Risk Assessment – Alton Manor Community Centre

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Building Construction** |  |  |  |  |
| **Hazard –** anything that could cause harm. E.g. equipment or conditions**Risk –** the chance that someone will be harmed by the hazard. | **Control –** All supervisors/Leaders to carry out a visual inspection of the building prior to each use.Any hazards identified should be assessed and managed appropriately. If necessary the Group Executive Committee should be notified at the earliest opportunity.  | Prior to each session | Person in charge of session | Continuous |
| **Roof Access** **Risk –** Falling through the roof, debris falling on users. | **Control –** No ready access to the roof. **Further Control measures -** Should access be necessary, professional assistance should be sought. Use of crawling boards, put up danger signs, no access to the internal building whilst person(s) on roof.Hard hats and safety boots to be worn.  | When access required | Person accessing roof | When access required |
| **Windows –** Broken glass or forced entry**Risk –** the chance someone will be harmed by the broken glass | **Control –** Visual inspection of the windows prior to use. Control activities to lessen the risk of breakage (Do not use heavy balls etc.)**Further Control Measures –** Consider the use of toughened glass or wire mesh | Prior to and during each sessionEvaluate in 3 months | Person in charge of sessionD. Barnes | Continuous |
| **Blocked drainpipes & gutters****Risk –** Slippery ground, worse if frozen | Regular inspection and cleaning out, seek professional help if necessary**Further control measures –** All supervisors/leaders to carry out a visual inspection prior to use | Prior to each session | Persons in charge of session | Continuous |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Access to site –** Damage to site, loss of facilities | **Control –** Secure fencing is erected around the perimeter, access is via two gates (one pedestrian, one vehicular).Security lighting is fitted on the outside of the building and above each door.**Further Control Measures –** Visual examination to take place prior to each session Additional security lighting to be installed on and around the storage container | DoneContinuousWithin 3 months | C. HallsworthPerson in charge of session A. Gee | April 15Continuous |
| **Services** |  |  |  |  |
| **Water** **Risk –** Leaks , blockages and burst pipes  | **Control –** Visual inspection and pipes lagged **Further Control Measures** - Check regularly, ensure taps are turned off after each session  | DoneContinuous | B&KPerson in charge of session | At installationContinuous |
| **Sewer and Waste****Risks –** Leaks, blockages and burst pipes | **Control –** Regular inspection | Continuous | D. Barnes | Continuous |
| **Water boiler & heaters****Risk –** Loss of use, hot heaters | **Control –** Water boiler installed by competent personsAppropriate heaters and guards fitted in each room**Further Control Measures –** Regular maintenance by competent person | DoneDoneAnnually  | B&KD.BarnesC. Hallsworth | At installation13/04/15 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Electricity****Risk –** Electrocution, fire **Trailing leads****Risk -** Tripping | **Control –** Main supply to site and building by competent persons.Additional electrical work completed by a qualified electrician**Further control measures –** Obtain installation certificates for all electrical work carried out so farAll electrical items within building to be PAK tested by qualified personAny additional electrical work to be carried out by qualified person and relevant certificates obtained. Isolate supply as necessary.Regular inspection of leads & plugs, remove anything sub-standardEnsure power leads are not pulled tight when connected to sockets and do pose a trip hazard to users | Feb 15When required15/06/1515/06/15When requiredContinuousContinuous | Southern Electric & B&KM. GeeM.GeeM. GeeM.GeePerson in charge of session Person in charge of session | Feb 15ContinuousContinuous |
| **Lighting****Risk –** Injuries caused by falling/broken lights  | **Control –** All lights are covered by protective casing**Further control measures –** Check the fluorescent lights and casing are of a shatterproof design and replace if necessary | 13/04/1515/06/15 | D. BarnesD. Barnes | 13/04/15 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Entrances & Exits** |  |  |  |  |
| **Obstructions****Risks –** Unable to operate doors in an emergency.Trips & FallsPoor lightingUneven Surfaces | **Control –** Ensure fire doors are unlocked, clear at all times. Check outside areas too. Remove any trip and fall hazards immediately. Report any deficiencies of surface or lighting. Correct emergency exit signage in place & Ensure good lighting (including emergency lighting) on exit routes Each section to practice a fire drill at least once a term (vary escape route)**Further control measures –** Fire door in rear door to be re-hinged so that it opens the opposite way  | ContinuousDone 13/4/15Each term01/09/15 | Person in charge of sessionD.BarnesSection LeaderH.Roberts | Continuous13/4/15October 2016 |
| **Storage** |  |  |  |  |
| **Combustible Materials****Risk –** Fire**Rubbish – Risk -** Disease/Vermin**Cleaning fluids/equipment –** **Risk –** Poisoning**Store Room (Tables & Chairs)****Risk –** Injury caused by falling items | **Control**Careful storage in containers. Remove other potential ignition sources Remove all rubbish, store food in appropriate containers or remove altogether where possible.Use outside refuse bins provided, contract with AVBC. Items stored in fridge only to be kept for the time their use is required. Remove/dispose from fridge after use. Cleaning fluids to be kept in cupboard under sink.**Further control measure** - fit child safety lock to cupboardChairs and tables to be stacked in a tidy manner. The tables stood on end, legs folded in. Chairs to be stacked on top of each other, no more than 8 chairs per stack  | ContinuousContinuousContinuous17/05/15Continuous | Person in charge of sessionPerson in charge of sessionR.CarlisleD.BarnesPerson in charge of session | ContinuousContinuousContinuousContinuous |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Kitchen** |  |  |  |  |
| **Sharp Objects****Risks – Cuts****Food & Drink****Risks –** Food poisoning, vermin, slipping on spills and scalds from boiling water. | **Control Measures –** Control access to knives and put them away in kitchen drawers provided after use.Reduce use of breakable glasses and cups. Dispose of broken glass or cups carefully (wrap in newspaper) and put straight into outside bins.Avoid leaving food in the premises where possible, remove waste to outside bins. Ensure basic hygiene practices are followed.Dispose of out of date items immediately.Clean up spills promptly using equipment provided (mop, bucket & cloths).Control access to kettle and hot water from taps.**Further control measures –** Purchase wet/slipper floor sign | ContinuousContinuous15/06/15 | Person in charge of sessionPersons in charge of sessionC. Hallsworth | ContinuousContinuous |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Toilets/Washrooms** |  |  |  |  |
| **Bacteria****Risk –** Disease | **Control Measures**Regular inspection and cleaning of facilities Good supply of toilet paper, soap, hand drying facilities, emptying of bins.Cleaner employed for weekly cleaning of facilities | Weekly | R. Carlisle | Weekly |
| **Rooms** |  |  |  |  |
| **Trips****Risk –** Injury caused by faulty/loose carpet**Risk** - Fire | **Control Measures**Regular inspection of the carpets for “lifting” paying particular attention to the joins in the carpets and doorways.Separate Fire Risk assessment management plan completed Test of fire alarms, smoke alarms and visual inspection of fire extinguishers and fire blankets on a monthly basis.Annual contract for professional inspection of fire extinguishers and fire blankets**Further control measures –** Users to sign that they have read the fire risk assessment plan and that they are aware of the roles and responsibilities.  | Weekly03/05/15MonthlyMarch 2015May 2015 | Person in charge of sessionD. BarnesD. BarnesC HallsworthD.Barnes (Scouts) & A. Gee (other users)  | WeeklyMay 15April 2015March 2015 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Car Park & Outdoor areas** |  |  |  |  |
| **Car Park****Risk –** Injury to children & adults by cars driving in car park**Concrete area at rear of building****Risk –** Injuries caused by disposed of objects (glass etc)**Surrounding Land (Rubbish, uneven land)****Risk –** fire, trips, cuts | **Control Measures**Speed restricted to 5mph within the car park. Warning Signs erected on the front gates warning users of speed and children.When children are using the car park for activities the double gates are to be closed preventing vehicular accessThe pedestrian gate to be used when arriving or leaving the centre on foot, both gates to be unlocked. Person in charge of session to ensure users are aware that foot traffic is by the pedestrian gateArea to be inspected prior to use and foreign objects disposed of.Walk and assess the area monthly, remove rubbish and hazardsLand at the side of the building next to the Carpet shop/florists out of bounds to children. Access by adults is on a “needs” basis only | April 2015ContinuousContinuousMay 2015ContinuousMonthlyContinuous | C. HallsworthPerson in charge of sessionPerson in charge of sessionPerson in charge of sessionPerson in charge of sessionD.Barnes Person in charge of session | April 2015ContinuousContinuousMay 15ActivityApril 2015Continuous |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Gas cylinders & appliances** |  |  |  |  |
| **Risk –** Leaks, fire, explosion | **Control Measures**Gas cylinders are stored in an approved locked gas cage, in an open area and free of combustible material, not below ground level and away from drains.Appropriate signage on the gas cageCylinders segregated between empty and fullAppliances to be visually inspected prior to use, paying particular attention to the hose and connections. Keep spares readily available**Further control measures –** Annual inspection of gas appliances by qualified person | March 15March 15March 15Each use30/06/15 | M. FieldM. FieldM. FieldPerson in charge of sessionM. Field | March 15March 15March 15Each use |
| **Camping Store** |  |  |  |  |
| **Risk –** TentsRotting, mildew Lifting heavy kitStoring at height | **Control Measures**A designated quartermaster appointed by the Scout GroupEnsure all kit is put away clean, dry and tidily.Break down into manageable amounts, work together. Do not expect Cubs, Scouts and adults to lift things that are too heavy, however willing.Put heavy things down low, light things higher. Check steps/ladders are in a good state of repair. **Further control measures –** Installation of lighting to the container & access to a 13amp power socket | March 15When usedWhen usedApril 15July 2015 | M.FieldPerson in charge of sessionPerson in charge of sessionM. FieldM.Field | March 15When usedWhen usedApril 15 |
| Hazard identified, risks arising and persons at risk | How is the risk controlled?What further controls are needed? | Date to be done | Person Responsible | Date completed |
| **Insurance -**  |  |  |  |  |
| **Risk –** Protection againstliability, theft, damage & injury | **Control Measures**1st Alton Manor Scout Group is insured by “Unity Scout Insurance Services” for building, members, helpers and occasional helpers, kit and equipment and public liability**Further Control Measures** Speak to Unity to see if extra insurance is required for employees (Cleaner) and for Community use | June 2014May 15 | D. BarnesD.Barnes | Renewal June 15 |
| **Additional Comments** |
| All hazards, breakages, faults and damages should be reported to the Group Secretary, Christine Hallsworth on 01773 828559 for dissemination to the appropriate person for rectification work.The accident reporting book is to be kept in the kitchen drawer and completed for all “relevant” accidents. The first aid kit will be fitted to the kitchen wall. |
| **This risk assessment covers Alton Manor Community Centre, it DOES NOT cover activities that take place at the centre. All activities that take place at the centre MUST be subjected to a risk assessment generic to the activity.** |
| Date of next assessment | May 2017 |
| Assessment Frequency | Annually |
| Date of assessment: | 4th May 2016 | Signed: | Darren Barnes Group Scout Leader |